|  |
| --- |
| **SOOW Cables** |

|  |  |
| --- | --- |
|  | SOOW cables maintain excellent flexibility in cold temperatures. They are ozone, water and weather resistant. They have a high heat resistance as well as being resistant to oils, acids and chemicals. In addition, they are excellent to abrasion and cut resistance. |
| |  |  | | --- | --- | | Conductor: | Bare Copper | | Insulation: | Ethylene Propylene Diene Monomer Rubber (EPDM) | | Jacket: | Neoprene | | Temp Rating: | 90°C | | Voltage Rating: | 600 Volts R.M.S. | | Color Code: | See Chart BCC-2 | | |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Blake Part Number** | **AWG** | **Number of Conductors** | **Stranding** | **Insulation** | **Jacket (inches)** | **O.D. (Inches)** | **AMPS** |
| **BCB-8483** | 8 | 3 | 65 x 26 | 0.050 | 0.060 | 0.700 | 40 |
| **BCB-8484** | 8 | 4 | 65 x 26 | 0.050 | 0.060 | 0.785 | 35 |
| **BCB-8485** | 8 | 5 | 65 x 26 | 0.050 | 0.060 | 0.830 | 35 |
| **BCB-8463** | 6 | 3 | 101 x 26 | 0.050 | 0.060 | 0.780 | 55 |
| **BCB-8464** | 6 | 4 | 101 x 26 | 0.050 | 0.080 | 0.845 | 45 |
| **BCB-8465** | 6 | 5 | 101 x 26 | 0.050 | 0.080 | 0.950 | 45 |
| **BCB-8442** | 4 | 2 | 119 x 25 | 0.050 | 0.080 | 0.865 | 70 |
| **BCB-8443** | 4 | 3 | 119 x 25 | 0.050 | 0.080 | 0.925 | 70 |
| **BCB-8444** | 4 | 4 | 119 x 25 | 0.050 | 0.080 | 1.000 | 60 |
| **BCB-8445** | 4 | 5 | 119 x 25 | 0.050 | 0.080 | 1.090 | 60 |
| **BCB-8423** | 2 | 3 | 119 x 23 | 0.600 | 0.080 | 1.055 | 95 |
| **BCB-8424** | 2 | 4 | 119 x 23 | 0.600 | 0.080 | 1.100 | 80 |
| **BCB-8425** | 2 | 5 | 119 x 23 | 0.600 | 0.080 | 1.435 | 80 |