|  |
| --- |
| **SOOW Cables** |

|  |  |
| --- | --- |
|  | SOOW cables maintain excellent flexibility in cold temperatures. They are ozone, water and weather resistant. They have a high heat resistance as well as being resistant to oils, acids and chemicals. In addition, they are excellent to abrasion and cut resistance. |
| |  |  | | --- | --- | | Conductor: | Bare Copper | | Insulation: | Ethylene Propylene Diene Monomer Rubber (EPDM) | | Jacket: | Super Vu-Tron® III | | Temp Rating: | 90°C | | Voltage Rating: | 600 Volts R.M.S. | | Color Code Chart: | See Chart BCC-2 | | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Blake Part Number** | **AWG** | **Number of Conductors** | **Stranding** | **Insulation** | **O.D. (Inches)** | **AMPS** |
| **BCB-8716** | 16 | 5 | 26 x 30 | 0.030 | 0.495 | 5.6 |
| **BCB-8717** | 16 | 6 | 26 x 30 | 0.030 | 0.520 | 5.6 |
| **BCB-8718** | 16 | 7 | 26 x 30 | 0.030 | 0.550 | 4.9 |
| **BCB-8719** | 16 | 8 | 26 x 30 | 0.030 | 0.575 | 4.9 |
| **BCB-8720** | 16 | 10 | 26 x 30 | 0.030 | 0.605 | 3.5 |
| **BCB-8721** | 16 | 12 | 26 x 30 | 0.030 | 0.605 | 3.5 |
| **BCB-8722** | 16 | 14 | 26 x 30 | 0.030 | 0.660 | 3.5 |
| **BCB-8723** | 16 | 16 | 26 x 30 | 0.030 | 0.705 | 3.5 |
| **BCB-8724** | 16 | 18 | 26 x 30 | 0.030 | 0.760 | 3.5 |
| **BCB-8725** | 16 | 20 | 26 x 30 | 0.030 | 0.795 | 3.5 |
| **BCB-8726** | 16 | 22 | 26 x 30 | 0.030 | 0.855 | 3.1 |
| **BCB-8727** | 16 | 24 | 26 x 30 | 0.030 | 0.901 | 3.1 |
| **BCB-8728** | 16 | 27 | 26 x 30 | 0.030 | 0.920 | 3.1 |
| **BCB-8729** | 16 | 30 | 26 x 30 | 0.030 | 0.925 | 3.1 |
| **BCB-8730** | 16 | 36 | 26 x 30 | 0.030 | 1.050 | 2.8 |
| **BCB-8731** | 16 | 37 | 26 x 30 | 0.030 |  |  |
| **BCB-8732** | 16 | 40 | 26 x 30 | 0.030 |  |  |